[CONTROLS]
Go Back\Cancel=BUTTON_B
Select\Accept=BUTTON_A
Insert Letter=BUTTON_BLACK
Delete Letter=BUTTON_WHITE
Cycle Down=BUTTON_DPAD_D
Cycle Up=BUTTON_DPAD_U
[TEXT]
PLAYER

Player Name:  This will be the driver name for  the selected car.

Parachute: Allows the player to select whether the parachute will be opened automatically or manually.

Stage: Allows the player to choose if the car will automatically pre-stage and stage before a race. If Auto is selected, the player will not control the car until the player disengages the autostage.

Dashboard: The dashboard in IHRA is represented as a cluster  of gauges that "float" on top of the 3D display. This  setting allows the player to customize the gauges that are displayed. Any item checked will be displayed.

Speedometer: Indicates the speed of the vehicle.

Tachometer: Indicates the RPM of the engine.

Oil pressure: Indicates the oil pressure. A low oil pressure is an  indicator of engine problems.

Oil temperature: Indicates the temperature of the oil. A high temperature indicates a problem with the engine.

Water temperature: Indicates the temperature of the water that is used as an engine coolant. A high temperature indicates  a problem. 

Transmission temperature: Indicates the temperature of the transmission. A high temperature indicates that the clutch may be slipping too   much or that an improperly sized torque converter is being used.

Shift light: A player definable light that comes on at an RPM level. IHRA allows two different shift points to be selected by the player.

Gear indicator: Indicates the current gear.

Trans-brake indicator: Indicates that the trans-brake is engaged. The trans-brake will prevent torque from being transferred to the wheels by locking the transmission in 1st and reverse gears at the same time.

Three-step indicator : Indicates the state of the three-step. The three-step is a rev limiter used to prevent over-revving the engine.

Line-lock indicator: Indicates that the line-lock is engaged. The line-lock will lock the brakes on only the front tires, allowing the rear   tires to rotate freely. Line-lock is used primarily for doing  a burnout.

Nitrous Indicator: This indicates when nitrous oxide injection is activated.

Christmas Tree display: This is the starting light display. The display will be on the left.

Tire traction: This indicates the temperature of the tires and its  effect on the force applied relative to how much the tires  can withstand. As temperature increases, the color on   the graph will change. Blue is cold, green is optimal,   yellow means you are approaching above optimal  temperature, red indicates overheated tires.

Distance gauge: Before a race begins, the distance gauge indicates the distance to the start line (and pre-stage light).
