[CONTROLS]
Go Back\Cancel=BUTTON_B
Select\Accept=BUTTON_A
Cycle Down=BUTTON_DPAD_D
Cycle Up=BUTTON_DPAD_U
Slider Left=BUTTON_DPAD_L
Slider Right=BUTTON_DPAD_R
[TEXT]
DELAY BOX

The delay box is a device used to program a specific delay from the release of the car to the actual launch of the car. The box can be triggered off of several devices:
Brake
Trans-brake
Line-lock
Two-step

The box can be set to the following types:
One shot Cross-over top light
One shot Cross-over bottom light
One shot Top light
One shot bottom light
Two shot Cross-over top- top light
Two shot Cross-over bottom- top light
Two shot Cross-over top- bottom light
Two shot Cross-over bottom- bottom light
Two shot top light- bottom light
Off
The box delay is specified in hundredths of seconds.
